## OFFER FORM ACTED [AFGHANISTAN]

**Tender N° T/02FIU/BQV/E24/Kabdul/11/06**

**Order ID:**

**Date: 11/06/2024**

## To be Filled by Bidder (COMPULSORY)

|  |  |
| --- | --- |
| **Company’s Name**  **(as per registration documents)** |  |
| **Company Authorized Representative’s Name**  **(as per registration documents or duly signed Power of Attorney)** |  |
| **Company Registration Number** |  |
| **Registration body** |  |
| **Company’s mailing address**  **Shop/Office/Building No**  **Street name**  **City**  **Governorate/province/district**  **Country** |  |
| **Commercial representative for the bid**  **(if different from authorized representative)** |  |
| **Phone contact number**  **Landline**  **Mobile No** |  |
| **Email address** |  |

I undersigned (to be filled in by the Bidder) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

agree to provide ACTED, non-profit NGO, with items answering the following specifications, according to the general conditions and responsibilities that I engage myself to follow.

Please fill in the following tables, one for each lot:

* If the tender is divided into lots, the Bidder may bid for one or all lots. Each lot may be subject to a separate contract and the quantities indicated for the different lots cannot be divided.
* The Bidder must offer all items & quantities indicated for each lot. Bids for part of a lot only will not be considered.
* If the Bidder is awarded more than one lot, a single contract may be concluded for each lot.

**Project Specification:**

This project includes the rehabilitation of the main building and some spare parts including carpentary, wiring, painting and masonary.

**Specification of Estimate and Bid:**

1.This estimate provides for all labour, material transport, tools, equipment’s and method of construction/rehabilitation and any other necessary to be incurred for the construction part and included overhead & profit for this whole process and site guidance given by the engineering representative

**BoQ for Rehabilitation of Desing Center Kabul Darulaman office, Jaye Rayes**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SN** | **Description of work or (Item & Specification)** | **Quantity** | **Unit** | **Unit Cost** | **Total (AFA)** |
| ***1*** | *Construction PCC Concrete with sandy gravel for Roof with 7cm thickness , M150 (1:2:4) the cement is fresh, the sand is washed, the water is clean, the proportion of cement-sand is considered, the work is complete with all required activities at least 7 days curing is required according to instruction of ACTED Engineer.* | *13.30* | *m3* |  |  |
| ***2*** | *Construction PCC Concrete with crash gravel for around the Building Side Walk with 3cm thickness , M150 (1:2:4) the cement is fresh, the sand is washed, the water is clean, the proportion of cement-sand is considered, the work is complete with all required activities at least 7 days curing is required according to instruction of ACTED Engineer.* | *4.74* | *m3* |  |  |
| ***3*** | *Construction of Brick masonry on Roof & three Column (35x 60x260cm) with cement & sand mortar M:250 (1:4) burnt brick with size of (7x11x23)cm will be used, the proportion of cement-sand is considered, at least-7 days curing with bringing of construction Materials from the Main Gate. complete with all related activities according to instruction of ACTED Engineer,.* | *3.20* | *m3* |  |  |
| ***4*** | *Supply and installation of Isogamy (4mm) Best quality available in the market the weight of one solander 10m should be 42kg & the sample should be approved by ACTED engineer before installation the Isogam should be from one company & not old more the 6month. Professional Person need to installed the isogam & 15 years guaranty is required in written. The work is complete with transportation cleaning of roof & installation.* | *244.00* | *m2* |  |  |
| ***5*** | *Construction of Roof excavation all existing soil & doing of Mud work leveling of roof & patriation of Roof in 5 Part, every part Should have suppurate Gutter the work should be professionally complete with all related activities according to instruction of ACTED Engineer.* | *210.00* | *m2* |  |  |
| ***6*** | *Installation best quality of Plastic Sheet on the Roof before pouring of concrete Vith all related work according to instruction of ACTED Engineer* | *210.00* | *m2* |  |  |
| ***7*** | *Supply &installation of Chinese Plastic Flat on Celling best quality available in the Market with installation & transportation complete work is required according to instruction of Acted Engineer* | *90* | *m2* |  |  |
| ***8*** | *Excavation of cylinder sewerage underground Septic tank 1m/6m with all related activities complete according to instruction of ACTED Engineer PCC ring for sewerage tank ( dia = 90cm , height = 50cm, thickness 6cm with one RCC cover according to the Drawing. The work is complete with Transportation & installation until end according to instruction of ACTED Engineer.* | *6.00* | *m* |  |  |
| ***9*** | *Cement & sand Plastering out side walls around the building & three Column with all necessary activities according to instruction of ACTED Engineer complete work is required according to the site need. Demolish of Existing plaster from damages Area of Wall.  Plastering should be flat with smooth finishing at the end high quality plastering is required sand should be acceptable for site engineer.* | *54.50* | *m2* |  |  |
| ***10*** | *Supply & installation one wooden Door (2.15x1.40) according to the Drawing with oil painting & wariness painting complete according to instruction of ACTED Engineers* | 3.0 | *m2* |  |  |
| ***11*** | *Supply & installation one Lock best quality for Doors قفل مغزی دروازه* | 10.0 | *Pcs* |  |  |
| ***12*** | *Supply & installation one Lock best quality for cupboard قفل انواری* | 5.0 | *Pcs* |  |  |
| ***13*** | *Supply & installation one Handle best quality for Drawer & Windows دستگیر* | 10.0 | *Pcs* |  |  |
| ***14*** | *Supply & installation one Magnet for cupboard مقناطیس* | 10.0 | *Pair* |  |  |
| ***15*** | *Supply & installation one Strap for cupboard چپراست* | 10.0 | *Pair* |  |  |
| ***16*** | *Supply & installation one Air conditioner هواکش* | 2.0 | *Pcs* |  |  |
| ***17*** | *Supply & installation one handle for Window دستگیر کلکین* | 6.0 | *Pcs* |  |  |
| ***18*** | *Supply & installation one Cup of Stone کپ بخاری* | 4.0 | *Pcs* |  |  |
| ***19*** | *Supply & installation one Net for Windows جالی* | 10.0 | *Pcs* |  |  |
| ***20*** | *PCC 6inch pipe for stove place نل بخاری کانکریتی* | 5.0 | *Pcs* |  |  |
| ***21*** | *Gypsum & soil plastering of inside walls with (Gypsum & Soil) according to the site need with all necessary activities according to instruction of ACTED Engineer complete work is required. Demolish of Existing plaster from damages Area of Wall.  Plastering should be flat with smooth finishing at the end high quality plastering is required send should be acceptable for site engineer.* | *59.50* | *m2* |  |  |
| ***22*** | *Supply installation of two bathroom complete sewerage system & new Water network system with installation of commodes, drainage, fashion set, according to the site need. The excavation & back filling of pipe trench to water Tank & septic tank according to the site. installation of water tank with insulation & cloth cover complete work is required. Supply & installation of I Beam (140x70x5mm) (95Kg/m) for bottom of water tank 2pcs (3m) including installation & transportation* | *1.00* | *Lump sum* |  |  |
| ***23*** | *Supply & installation of two bathroom floor tile work with all necessary activities complete according to instruction of ACTED Engineer best quality of tile available in the market is required. Installation Work of 8m2 Marble l stone on Kitchen floor according to site need complete work is required.* | *15.00* | *m2* |  |  |
| ***24*** | *Supply & installation of Vertical Gutter from Iron sheet 24 Gage (0.5)mm with size of (12X8cm) with Iron Plate for installation of gutter on the roof with all necessary work complete according to the instruction of ACTED complete with installation. The steel materials should be checked and approved by ACTED Engineer before installation.* | *19.20* | *m* |  |  |
| ***25*** | *Plastic Painting 100% of Outside Building Complete with Best quality paint available in the market with all necessary work & materials complete with smooth finishing at the end according to the instruction of ACTED Engineer.* | *66.00* | *m2* |  |  |
| ***26*** | *Plastic Painting 50% of inside the Building with Best quality paint available in the market with all necessary work & materials complete with smooth finishing at the end according to the instruction of ACTED Engineer.* | *241.00* | *m2* |  |  |
| ***27*** | *Oil Painting of all Doors & Windows inside & Out side of Building with cupboards complete, Best quality paint available in the market with all necessary work & materials complete with smooth finishing at the end according to the instruction of ACTED Engineer.* | *152.00* | *m2* |  |  |
| ***28*** | *Supply & installation of 4mm best quality Glass for Door and Windows around the building with transportation.* | *5.00* | *m2* |  |  |
| ***29*** | *Supply & installation of Electrical Equipment Switch 10-pcs best quality available in the market  Socket 10-pcs best quality available in the market  LED Light (60x60)cm 5Pcs best quality available in the market  Light 10-pcs best quality available in the market* | *1.00* | *Lum* |  |  |
| ***30*** | *Supply & Installation of entrance steel Door according to the Drawing & technical Specification with 2layers oil paint & 2layer unrest painting & required activities according to instruction of ACTED Engineers.  The steel materials should be checked and approved by ACTED Engineer before installation. Supply & installation of I Beam (140x70x5mm) (95Kg/m) for lintel of steel door  2pcs (2m) with installation & transportation* | *1.00* | *Lum* |  |  |
| ***31*** | *Rehabilitation of 2 entrance Main Get Steel Door with oil Painting & all necessary equipment & related activities according to the site need.* | *1.00* | *Lum* |  |  |
| ***32*** | *Rehabilitation and straw mad Plastering around the building with all necessary activities according to instruction of ACTED engineer complete work is required according to the site need.  Plastering should be flat with smooth finishing at the end high quality plastering is required sand should be acceptable for site engineer.* | *59.50* | *m2* |  |  |
| ***33*** | *Cleaning of the basement from Soil & cleaning of the building from extra construction materials complete work is required.* | *1.00* | *Lump Sum* |  |  |
| Grand Total | | | | |  |

Workplan:

Please attach a detailed work plan demonstrating your ability to fulfil ACTED’s expectations.

Bidder’s Conditions:

|  |  |  |
| --- | --- | --- |
|  | General conditions recommended by ACTED | General conditions offered by Bidders (if different) |
| Validity of the offer | Six months |  |
| Terms of payment | Negotiable |  |

Name of Bidder’s Authorized Representative :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Authorized signature and stamp: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_